<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="60.96" y1="22.86" x2="82.53" y2="22.86" width="0" layer="20"/>
<wire x1="82.53" y1="22.86" x2="82.53" y2="51.74" width="0" layer="20"/>
<wire x1="82.53" y1="51.74" x2="60.96" y2="51.74" width="0" layer="20"/>
<wire x1="60.96" y1="51.74" x2="60.96" y2="22.86" width="0" layer="20"/>
</plain>
<libraries>
<library name="Capacitor">
<description>&lt;B&gt;Capacitors - Fixed, Variable, Trimmers</description>
<packages>
<package name="CAPC3216X135">
<description>Chip, 3.20 X 1.60 X 1.35 mm body
&lt;p&gt;Chip package with body size 3.20 X 1.60 X 1.35 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-1206">
<description>&lt;h3&gt;LED 1206 SMT&lt;/h3&gt;

1206, surface mount. 

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: &lt;/li&gt;
&lt;li&gt;Area: 0.125" x 0.06"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="6_PIN_SERIAL_TARGET_SIDE_RA_SMT">
<description>&lt;h3&gt;6 pin Serial Target - Right Angle  SMT&lt;/h3&gt;
Package for devices meant to mate to an FTDI connector. 
&lt;p&gt; tDocu shows pin location. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;6_Pin_Serial_Target&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Resistor">
<description>&lt;B&gt;Resistors, Potentiometers, TrimPot</description>
<packages>
<package name="RESC3216X70">
<description>Chip, 3.20 X 1.60 X 0.70 mm body
&lt;p&gt;Chip package with body size 3.20 X 1.60 X 0.70 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="attiny_fab">
<packages>
<package name="SOIC8_SA_SST_MCH">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="Capacitor" package="CAPC3216X135" value="">
<attribute name="CATEGORY" value="Capacitor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value=""/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE_RATING" value=""/>
</element>
<element name="D1" library="SparkFun-LED" package="LED-1206" value="GREEN">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-00862"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="6_PIN_SERIAL_TARGET_SIDE_RA_SMT" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08971"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="Resistor" package="RESC3216X70" value="">
<attribute name="CATEGORY" value="Resistor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="RATING" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="Fixed"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="attiny_fab" package="SOIC8_SA_SST_MCH" value="ATTINY412-SSNR">
<attribute name="BUILT_BY" value="EMA_Molly"/>
<attribute name="COPYRIGHT" value="Copyright (C) 2018 Accelerated Designs. All rights reserved"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ATTINY412-SSNR"/>
<attribute name="NAME"/>
<attribute name="SOURCELIBRARY" value="Microchip_2019-08-23_25"/>
<attribute name="VALUE"/>
<attribute name="VENDOR" value="Microchip"/>
</element>
</elements>
<signals>
<signal name="VDD">
<contactref element="J1" pad="4"/>
<contactref element="U1" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="TX">
<contactref element="U1" pad="2"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="RX">
<contactref element="U1" pad="3"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="UPDI">
<contactref element="U1" pad="6"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="4"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="R1" pad="1"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="GND">
<contactref element="D1" pad="C"/>
<contactref element="J1" pad="6"/>
<contactref element="U1" pad="8"/>
<contactref element="C1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
